1. Purpose
   1. This work instruction describes the process for replacing the label of the MX5 Centrifuge
   2. These repair instructions are valid for Revision G of the MX5 Centrifuge (101072-G and 100900-G) as well as any previous revisions that are compatible with the label (100929).
2. Equipment/Software

|  |  |  |  |
| --- | --- | --- | --- |
| ITEM # | PART # | DESCRIPTION | QTY. |
| 1 | 100929 | UI Label; raised button pads; blue & white; MX5 Centrifuge | 1 |

1. Instructions
   1. Confirm that all necessary components are present to complete the conversion.
   2. Carefully remove the damaged front label from the unit.

A grey box with a circular object

Description automatically generated

* 1. Replace the label with a new 100929 label.

A grey box with a circular object

Description automatically generated

* 1. Turn on the unit and verify all buttons are functional with the new label.